|  |  |
| --- | --- |
| Weight (LBS) | 1.59 |
| UOM | EA |
| UPC | 062503701013 |
| CFM | 130 |
| Product Color | White |
| Power Supply (V) | 12 V |
| Speed Settings | 3 |
| Current Draw on Low | 0.15A |
| Current Draw on High | 0.27A |
| Airflow on Low | 100 CFM |
| Airflow on High | 130 CFM |
| Connection Type | Direct Wire |
| Limited Warranty | 2 Year |